Test Devlog

# MAINPROGT3

1. Change CARRIER\_FREQUENCE to 99999.9f.
2. ISM band works when Amateur band fails.
3. Change antenna NSS pin to 10 instead of 7.
4. Complete transmission failure.
5. Restarting the satellite delay time changed to 1 minute.
6. Satellite gets stuck when receiving transmissions.
   1. Increased delay between each receive invokes.
   2. Checked for malformed data in Communication router. (worked but unreliable)
   3. Checking received string for data (could be null).
   4. The receive function in a for loop seems to break see (<https://github.com/jgromes/RadioLib/issues/10>)
      1. Testing with increased delay.
   5. It was a memory issue, solved by making string and int lowest scope possible.